************* About the "05orche.mid" (Space Flight) **************

The "05orche.mid" (Space Flight) in the "SC-8850" folder is a 
Standard MIDI file (Format1) using 32-track/32-MIDI channels, and 
it cannot be played back correctly using a MIDI cable.
You should set your sequencer following the instructions below.

* Depending on the sequencing software, there is a case you cannot
play this song correctly.

The tracks in this song are set to the following tracks when you 
open the file.


	A01 - Violin1
	A02 - Violin2
	A03 - Viola
	A04 - Cello
	A05 - Contrabass
	A06 - Mild St R
	A07 - Mild St L
	A08 - Str Spiic.
	A09 - Timpani
	A10 - S.D.
	A11 - Quad Brs1
	A12 - Trumpet
	A13 - Piano
	A14 - Glocken
	A15 - Xylophon
	A16 - Tubular bell
	B01 - Piccolo
	B02 - Flute
	B03 - Oboe
	B04 - Clarinet
	B05 - Horn Rip&Fg
	B06 - Horn&Choir
	B07 - Orch Brass
	B08 - Orch Brs 2
	B09 - Trombone
	B10 - B.D&Cymbal
	B11 - Bass Tromb
	B12 - Tuba
	B13 - StOrch Brs2
	B14 - StOrch Brs3
	B15 - Harp R
	B16 - Harp L



You should set the 16 channels from A01-Violin1 to A16-Tubular 
bell to the output port A, and the 16 channels from B01-Piccolo 
to B16-Harp L to the output port B.


	A01-Violin1		-> A Port 1 CH
	A02-Violin2		-> A Port 2 CH
	A03-Viola		-> A Port 3 CH
	A04-Cello		-> A Port 4 CH
	A05-Contrabass		-> A Port 5 CH
	A06-Mild St R		-> A Port 6 CH
	A07-Mild St L		-> A Port 7 CH
	A08-Str Spiic.		-> A Port 8 CH
	A09-Timpani		-> A Port 9 CH
	A10-S.D.		-> A Port 10 CH
	A11-Quad Brs1		-> A Port 11 CH
	A12-Trumpet		-> A Port 12 CH
	A13-Piano		-> A Port 13 CH
	A14-Glocken		-> A Port 14 CH
	A15-Xylophon		-> A Port 15 CH
	A16-Tubular bell	-> A Port 16 CH
	B01-Piccolo		-> B Port 1 CH
	B02-Flute		-> B Port 2 CH
	B03-Oboe		-> B Port 3 CH
	B04-Clarinet		-> B Port 4 CH
	B05-Horn Rip&Fg		-> B Port 5 CH
	B06-Horn&Choir		-> B Port 6 CH
	B07-Orch Brass		-> B Port 7 CH
	B08-Orch Brs 2		-> B Port 8 CH
	B09-Trombone		-> B Port 9 CH
	B10-B.D&Cymbal		-> B Port 10 CH
	B11-Bass Tromb		-> B Port 11 CH
	B12-Tuba		-> B Port 12 CH
	B13-StOrch Brs2		-> B Port 13 CH
	B14-StOrch Brs3		-> B Port 14 CH
	B15-Harp R		-> B Port 15 CH
	B16-Harp L		-> B Port 16 CH


* For details on how to change the sequencing software's settings, 
refer to the owner's manual for your software.